Install file download link: http://down.avldiy.cn/down_server/HD512_DVD/AllDVD_OneFile/
---------------------------------------------------------------------------------------

Howto:
Copy "efk_hardware.dll" and "hahan.dll" file to "C:\Program Files\SweetLight" Directory or any other you install SweetLight Directory, nothing to setup, then can use SweetLight software control fixture with our HD512 box.
this software can support win7, 8 , 8.1 , 10, 11... x64 system.

if you have our 2 ~ 4 pcs HD512 box want combination 1024 ~ 2048 channels, can run any ForXXX.exe plugin to set box Number in your PC, in this Plugin "BoxNumber" select [2 1024 Channel] ~ [4 2048 Channel], close ForXXX, your PC will remember the Box Number, next time run ShowXpress, then can use 2~4 box.
if Combination 1024 ~ 2048 channels, HD512 Box must set Universe ID, can run TestDemo to check and setup Universe ID. 

Please Note: 
this DLL plugin maybe can support all above 9.3.8 x64 SweetLight version,
In same time, ForSweetLight plugin and this DLL plugin, this 2 kinds of plug-ins only choose one for use.



--------------------------Chinese--------------------------------------------------------
拷贝我们的"efk_hardware.dll" 和 "hahan.dll"  文件到 SweetLight 程序目录， "C:\Program Files\SweetLight" 
不需要任何设置就可以通过 SweetLight 软件加我们HD512盒子控制灯光了。
可以支持Win7, 8, 8.1, 10, 11...  x64 系统。

如果你有我们多个盒子进行组合，需要运行ForXXX软件设置盒子的个数，假设有2个的话，请选择[2 1024 Channel]，在新电脑中，这个设置只需要做一次。如果只是单个盒子，可以不用设置，多个盒子组合用的话，才需要设置。4个盒子组合2048通道的话请选择 [4 2048 Channel]进行设置，注意，如果只有单个盒子，请勿设置成多个盒子，否则会出现意想不到的结果。

敬请注意：
这个DLL插件支持所有SweetLight版本，欢迎使用。
ForSweetLight插件和DLL插件，2者只能选择其中一种使用，不能同时使用。


                         hahan
                     2023-08-24